ENS210 Temperature+Humidity Sensor
==================================

.. seo::
    :description: Instructions for setting up ENS210 temperature and humidity sensors
    :image: ens210.jpg
    :keywords: ENS210

The ``ENS210`` Temperature+Humidity sensor allows you to use your ENS210
(`datasheet <https://www.sciosense.com/wp-content/uploads/2021/01/ENS210.pdf>`__) i2c-based sensor with ESPHome.

.. figure:: images/ens210.jpg
    :align: center
    :width: 80.0%

    ENS210 Temperature & Humidity Sensor.

.. figure:: images/temperature-humidity.png
    :align: center
    :width: 80.0%

.. code-block:: yaml

    # Example configuration entry
    sensor:
      - platform: ENS210
        temperature:
          name: "Living Room Temperature"
        humidity:
          name: "Living Room Humidity"
        update_interval: 60s

Configuration variables:
------------------------

- **temperature** (**Required**): The information for the temperature sensor.

  - **name** (**Required**, string): The name for the temperature sensor.
  - **id** (*Optional*, :ref:`config-id`): Set the ID of this sensor for use in lambdas.
  - All other options from :ref:`Sensor <config-sensor>`.

- **humidity** (**Required**): The information for the humidity sensor

  - **name** (**Required**, string): The name for the humidity sensor.
  - **id** (*Optional*, :ref:`config-id`): Set the ID of this sensor for use in lambdas.
  - All other options from :ref:`Sensor <config-sensor>`.

- **update_interval** (*Optional*, :ref:`config-time`): The interval to check the sensor. Defaults to ``60s``.


See Also
--------

- :ref:`sensor-filters`
- :apiref:`ENS210/ENS210.h`
- `ENS210 Library <https://github.com/maarten-pennings/ENS210>`__  by `Maarten Pennings  <https://github.com/maarten-pennings>`__
- :ghedit:`Edit`
